Overview | Package | Class | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES

Packages
cnrg.itx.gtwy | The gateway is the interface where the computer and telephone networks can transfer voice data to one another. In the cnrg.itx.gtwy package, the software is configured to program Dialogic Corporation's D41/EPCI card. The Windows NT platform is necessary to use this software. It is important to note that the D41/EPCI channels are limited to servicing half-duplex connections only. In order to service a full-duplex connection, two channels are needed per session. A "line" is an abstraction of these two channels.
cnrg.itx.gtwy.pbx | This is stripped-down JTapi code for controlling a PBX, allowing outgoing calls.

Overview | Package | Class | Tree | Deprecated | Index | Help
PREV NEXT | FRAMES NO FRAMES